# Static Call Graph - [UKSI_TEST\UKSI_TEST.axf]

# Static Call Graph for image UKSI_TEST\UKSI_TEST.axf

#<CALLGRAPH># ARM Linker, 6190004: Last Updated: Tue Dec 16 17:45:13 2025

### Maximum Stack Usage = 364 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ MX_ADC1_Init ⇒ HAL_ADC_ConfigChannel ⇒ LL_ADC_SetOffset

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - BusFault_Handler from stm32g4xx_it.o(.text.BusFault_Handler) referenced from startup_stm32g431xx.o(RESET)
  - COMP1_2_3_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - COMP4_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - CORDIC_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - CRS_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - DMA2_Channel4_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - DMA2_Channel5_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - DMA2_Channel6_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - DMAMUX_OVR_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - DebugMon_Handler from stm32g4xx_it.o(.text.DebugMon_Handler) referenced from startup_stm32g431xx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - FDCAN1_IT0_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - FDCAN1_IT1_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - FMAC_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - FPU_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - FilterAverageInt_Init from filters.o(.text.FilterAverageInt_Init) referenced 2 times from filters.o(.text.FilterAverageInt_Init)
  - FilterAverageInt_Process from filters.o(.text.FilterAverageInt_Process) referenced 2 times from filters.o(.text.FilterAverageInt_Init)
  - FilterMedianInt_Init from filters.o(.text.FilterMedianInt_Init) referenced 2 times from filters.o(.text.FilterMedianInt_Init)
  - FilterMedianInt_Process from filters.o(.text.FilterMedianInt_Process) referenced 2 times from filters.o(.text.FilterMedianInt_Init)
  - HardFault_Handler from stm32g4xx_it.o(.text.HardFault_Handler) referenced from startup_stm32g431xx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - LPTIM1_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - LPUART1_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - MemManage_Handler from stm32g4xx_it.o(.text.MemManage_Handler) referenced from startup_stm32g431xx.o(RESET)
  - NMI_Handler from stm32g4xx_it.o(.text.NMI_Handler) referenced from startup_stm32g431xx.o(RESET)
  - PVD_PVM_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - PendSV_Handler from stm32g4xx_it.o(.text.PendSV_Handler) referenced from startup_stm32g431xx.o(RESET)
  - RCC_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - RNG_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - RTC_TAMP_LSECSS_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - Reset_Handler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - SAI1_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - SVC_Handler from stm32g4xx_it.o(.text.SVC_Handler) referenced from startup_stm32g431xx.o(RESET)
  - SysTick_Handler from stm32g4xx_it.o(.text.SysTick_Handler) referenced from startup_stm32g431xx.o(RESET)
  - SystemInit from system_stm32g4xx.o(.text.SystemInit) referenced from startup_stm32g431xx.o(.text)
  - TIM1_BRK_TIM15_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - TIM1_TRG_COM_TIM17_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - TIM1_UP_TIM16_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - TIM3_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - UART4_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - UCPD1_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - USART1_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - USART2_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - USART3_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - USB_HP_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - USB_LP_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - UsageFault_Handler from stm32g4xx_it.o(.text.UsageFault_Handler) referenced from startup_stm32g431xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32g431xx.o(.text) referenced from startup_stm32g431xx.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32g431xx.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __rt_entry
  - >> __scatterload
  [Address Reference Count : 1]
  - startup_stm32g431xx.o(.text)

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000001))
  [Calls]

  - >> _fp_init

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000034))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000006))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000010))

  __rt_lib_init_relocate_pie_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000035))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000027))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __main
  - >> __scatterload_rt2

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 364 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ MX_ADC1_Init ⇒ HAL_ADC_ConfigChannel ⇒ LL_ADC_SetOffset
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32g431xx.o(RESET)

  COMP1_2_3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  COMP4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  CORDIC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  CRS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  DMA2_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  DMA2_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  DMA2_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  DMAMUX_OVR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  FDCAN1_IT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  FDCAN1_IT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  FMAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  LPTIM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  LPUART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  PVD_PVM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  RTC_TAMP_LSECSS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  SAI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  TIM1_BRK_TIM15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  TIM1_TRG_COM_TIM17_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  TIM1_UP_TIM16_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  UCPD1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  USB_HP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  USB_LP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32g431xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32g431xx.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __aeabi_ldivmod (Thumb, 0 bytes, Stack size 24 bytes, llsdiv.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = __aeabi_ldivmod
  [Called By]
  - >> FilterAverageInt_Process

  _ll_sdiv (Thumb, 116 bytes, Stack size 24 bytes, llsdiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size unknown bytes, rt_memclr_w.o(.text))
  [Called By]

  - >> HAL_ADC_MspInit
  - >> MX_TIM1_Init
  - >> SystemClock_Config

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size unknown bytes, rt_memclr_w.o(.text), UNUSED)

  __rt_memclr_w (Thumb, 0 bytes, Stack size unknown bytes, rt_memclr_w.o(.text), UNUSED)

  _memset_w (Thumb, 74 bytes, Stack size 4 bytes, rt_memclr_w.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __aeabi_uldivmod (Thumb, 0 bytes, Stack size 48 bytes, lludivv7m.o(.text), UNUSED)
  [Called By]

  - >> _ll_sdiv

  _ll_udiv (Thumb, 240 bytes, Stack size 48 bytes, lludivv7m.o(.text), UNUSED)

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size unknown bytes, indicate_semi.o(.text), UNUSED)

  ADC_Calc (Thumb, 254 bytes, Stack size 32 bytes, uksi_calc_res.o(.text.ADC_Calc))
  [Stack]

  - Max Depth = 36
  - Call Chain = ADC_Calc ⇒ HAL_ADC_GetValue
  [Calls]
  - >> HAL_ADC_GetValue
  [Called By]
  - >> UKSI_Calc_Isolation

  ADC_ConfigCoef (Thumb, 130 bytes, Stack size 36 bytes, uksi_calc_res.o(.text.ADC_ConfigCoef))
  [Stack]

  - Max Depth = 36
  - Call Chain = ADC_ConfigCoef
  [Called By]
  - >> UKSI_Calc_Init

  ADC_ConfigFilter (Thumb, 118 bytes, Stack size 32 bytes, uksi_calc_res.o(.text.ADC_ConfigFilter))
  [Stack]

  - Max Depth = 52
  - Call Chain = ADC_ConfigFilter ⇒ FilterMedianInt_Init
  [Calls]
  - >> FilterAverageInt_Init
  - >> FilterMedianInt_Init
  [Called By]
  - >> UKSI_Calc_Init

  ADC_Disable (Thumb, 196 bytes, Stack size 24 bytes, stm32g4xx_hal_adc.o(.text.ADC_Disable))
  [Stack]

  - Max Depth = 28
  - Call Chain = ADC_Disable ⇒ LL_ADC_Disable
  [Calls]
  - >> HAL_GetTick
  - >> LL_ADC_Disable
  - >> LL_ADC_IsDisableOngoing
  - >> LL_ADC_IsEnabled
  [Called By]
  - >> HAL_ADCEx_Calibration_Start

  ADC_Enable (Thumb, 272 bytes, Stack size 24 bytes, stm32g4xx_hal_adc.o(.text.ADC_Enable))
  [Stack]

  - Max Depth = 28
  - Call Chain = ADC_Enable ⇒ LL_ADC_GetCommonPathInternalCh
  [Calls]
  - >> HAL_GetTick
  - >> LL_ADC_GetCommonPathInternalCh
  - >> LL_ADC_Enable
  - >> LL_ADC_IsEnabled
  [Called By]
  - >> HAL_ADC_Start

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32g4xx_it.o(.text.BusFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  DC_Enable (Thumb, 92 bytes, Stack size 12 bytes, uksi_dc_control.o(.text.DC_Enable))
  [Stack]

  - Max Depth = 12
  - Call Chain = DC_Enable
  [Called By]
  - >> UKSI_while

  DC_Init (Thumb, 88 bytes, Stack size 32 bytes, uksi_dc_control.o(.text.DC_Init))
  [Stack]

  - Max Depth = 120
  - Call Chain = DC_Init ⇒ HAL_TIM_OC_Start ⇒ TIM_CCxChannelCmd
  [Calls]
  - >> HAL_TIMEx_OCN_Start
  - >> HAL_TIM_OC_Start
  [Called By]
  - >> UKSI_Init

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32g4xx_it.o(.text.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  Error_Handler (Thumb, 14 bytes, Stack size 4 bytes, main.o(.text.Error_Handler))
  [Stack]

  - Max Depth = 4
  - Call Chain = Error_Handler
  [Called By]
  - >> HAL_ADC_MspInit
  - >> MX_TIM1_Init
  - >> MX_TIM17_Init
  - >> MX_ADC1_Init
  - >> SystemClock_Config

  FilterAverageInt_Init (Thumb, 128 bytes, Stack size 16 bytes, filters.o(.text.FilterAverageInt_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = FilterAverageInt_Init
  [Called By]
  - >> ADC_ConfigFilter
  [Address Reference Count : 1]
  - filters.o(.text.FilterAverageInt_Init)

  FilterAverageInt_Process (Thumb, 148 bytes, Stack size 32 bytes, filters.o(.text.FilterAverageInt_Process))
  [Stack]

  - Max Depth = 56
  - Call Chain = FilterAverageInt_Process ⇒ __aeabi_ldivmod
  [Calls]
  - >> __aeabi_ldivmod
  [Address Reference Count : 1]
  - filters.o(.text.FilterAverageInt_Init)

  FilterMedianInt_Init (Thumb, 170 bytes, Stack size 20 bytes, filters.o(.text.FilterMedianInt_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = FilterMedianInt_Init
  [Called By]
  - >> ADC_ConfigFilter
  [Address Reference Count : 1]
  - filters.o(.text.FilterMedianInt_Init)

  FilterMedianInt_Process (Thumb, 480 bytes, Stack size 36 bytes, filters.o(.text.FilterMedianInt_Process))
  [Stack]

  - Max Depth = 36
  - Call Chain = FilterMedianInt_Process
  [Address Reference Count : 1]
  - filters.o(.text.FilterMedianInt_Init)

  HAL_ADCEx_Calibration_Start (Thumb, 224 bytes, Stack size 32 bytes, stm32g4xx_hal_adc_ex.o(.text.HAL_ADCEx_Calibration_Start))
  [Stack]

  - Max Depth = 60
  - Call Chain = HAL_ADCEx_Calibration_Start ⇒ ADC_Disable ⇒ LL_ADC_Disable
  [Calls]
  - >> LL_ADC_IsCalibrationOnGoing
  - >> LL_ADC_StartCalibration
  - >> ADC_Disable
  [Called By]
  - >> UKSI_Calc_Init

  HAL_ADCEx_MultiModeConfigChannel (Thumb, 374 bytes, Stack size 152 bytes, stm32g4xx_hal_adc_ex.o(.text.HAL_ADCEx_MultiModeConfigChannel))
  [Stack]

  - Max Depth = 156
  - Call Chain = HAL_ADCEx_MultiModeConfigChannel ⇒ LL_ADC_IsEnabled
  [Calls]
  - >> LL_ADC_IsEnabled
  - >> LL_ADC_REG_IsConversionOngoing
  [Called By]
  - >> MX_ADC1_Init

  HAL_ADC_ConfigChannel (Thumb, 2024 bytes, Stack size 264 bytes, stm32g4xx_hal_adc.o(.text.HAL_ADC_ConfigChannel))
  [Stack]

  - Max Depth = 284
  - Call Chain = HAL_ADC_ConfigChannel ⇒ LL_ADC_SetOffset
  [Calls]
  - >> LL_ADC_SetCommonPathInternalCh
  - >> LL_ADC_SetChannelSingleDiff
  - >> LL_ADC_SetOffsetState
  - >> LL_ADC_GetOffsetChannel
  - >> LL_ADC_SetOffsetSaturation
  - >> LL_ADC_SetOffsetSign
  - >> LL_ADC_SetOffset
  - >> LL_ADC_SetSamplingTimeCommonConfig
  - >> LL_ADC_SetChannelSamplingTime
  - >> LL_ADC_REG_SetSequencerRanks
  - >> LL_ADC_GetCommonPathInternalCh
  - >> LL_ADC_INJ_IsConversionOngoing
  - >> LL_ADC_IsEnabled
  - >> LL_ADC_REG_IsConversionOngoing
  [Called By]
  - >> MX_ADC1_Init

  HAL_ADC_GetValue (Thumb, 14 bytes, Stack size 4 bytes, stm32g4xx_hal_adc.o(.text.HAL_ADC_GetValue))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_ADC_GetValue
  [Called By]
  - >> ADC_Calc

  HAL_ADC_Init (Thumb, 792 bytes, Stack size 40 bytes, stm32g4xx_hal_adc.o(.text.HAL_ADC_Init))
  [Stack]

  - Max Depth = 196 + Unknown Stack Size
  - Call Chain = HAL_ADC_Init ⇒ HAL_ADC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> LL_ADC_INJ_IsConversionOngoing
  - >> LL_ADC_SetCommonClock
  - >> LL_ADC_IsEnabled
  - >> LL_ADC_REG_IsConversionOngoing
  - >> LL_ADC_EnableInternalRegulator
  - >> LL_ADC_IsInternalRegulatorEnabled
  - >> LL_ADC_DisableDeepPowerDown
  - >> LL_ADC_IsDeepPowerDownEnabled
  - >> HAL_ADC_MspInit
  [Called By]
  - >> MX_ADC1_Init

  HAL_ADC_MspInit (Thumb, 154 bytes, Stack size 112 bytes, adc.o(.text.HAL_ADC_MspInit))
  [Stack]

  - Max Depth = 156 + Unknown Stack Size
  - Call Chain = HAL_ADC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> HAL_GPIO_Init
  - >> Error_Handler
  - >> __aeabi_memclr4
  [Called By]
  - >> HAL_ADC_Init

  HAL_ADC_Start (Thumb, 460 bytes, Stack size 40 bytes, stm32g4xx_hal_adc.o(.text.HAL_ADC_Start))
  [Stack]

  - Max Depth = 68
  - Call Chain = HAL_ADC_Start ⇒ ADC_Enable ⇒ LL_ADC_GetCommonPathInternalCh
  [Calls]
  - >> ADC_Enable
  - >> LL_ADC_REG_StartConversion
  - >> LL_ADC_GetMultimode
  - >> LL_ADC_REG_IsConversionOngoing
  [Called By]
  - >> UKSI_Calc_Init

  HAL_GPIO_Init (Thumb, 872 bytes, Stack size 44 bytes, stm32g4xx_hal_gpio.o(.text.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 44
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> HAL_TIM_MspPostInit
  - >> HAL_ADC_MspInit
  - >> MX_GPIO_Init

  HAL_GPIO_WritePin (Thumb, 44 bytes, Stack size 8 bytes, stm32g4xx_hal_gpio.o(.text.HAL_GPIO_WritePin))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_GPIO_WritePin
  [Called By]
  - >> MX_GPIO_Init

  HAL_GetTick (Thumb, 12 bytes, Stack size 0 bytes, stm32g4xx_hal.o(.text.HAL_GetTick))
  [Called By]

  - >> ADC_Enable
  - >> ADC_Disable
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCC_OscConfig

  HAL_IncTick (Thumb, 26 bytes, Stack size 0 bytes, stm32g4xx_hal.o(.text.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 48 bytes, Stack size 16 bytes, stm32g4xx_hal.o(.text.HAL_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ NVIC_EncodePriority
  [Calls]
  - >> HAL_InitTick
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_MspInit
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 136 bytes, Stack size 16 bytes, stm32g4xx_hal.o(.text.HAL_InitTick))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ NVIC_EncodePriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_SYSTICK_Config
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCC_OscConfig
  - >> HAL_Init

  HAL_MspInit (Thumb, 72 bytes, Stack size 16 bytes, stm32g4xx_hal_msp.o(.text.HAL_MspInit))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_MspInit
  [Calls]
  - >> HAL_PWREx_DisableUCPDDeadBattery
  [Called By]
  - >> HAL_Init

  HAL_NVIC_SetPriority (Thumb, 46 bytes, Stack size 32 bytes, stm32g4xx_hal_cortex.o(.text.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_NVIC_SetPriority ⇒ NVIC_EncodePriority
  [Calls]
  - >> __NVIC_SetPriority
  - >> NVIC_EncodePriority
  - >> __NVIC_GetPriorityGrouping
  [Called By]
  - >> HAL_InitTick

  HAL_NVIC_SetPriorityGrouping (Thumb, 16 bytes, Stack size 16 bytes, stm32g4xx_hal_cortex.o(.text.HAL_NVIC_SetPriorityGrouping))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_NVIC_SetPriorityGrouping ⇒ __NVIC_SetPriorityGrouping
  [Calls]
  - >> __NVIC_SetPriorityGrouping
  [Called By]
  - >> HAL_Init

  HAL_PWREx_ControlVoltageScaling (Thumb, 436 bytes, Stack size 20 bytes, stm32g4xx_hal_pwr_ex.o(.text.HAL_PWREx_ControlVoltageScaling))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_PWREx_ControlVoltageScaling
  [Called By]
  - >> SystemClock_Config

  HAL_PWREx_DisableUCPDDeadBattery (Thumb, 18 bytes, Stack size 0 bytes, stm32g4xx_hal_pwr_ex.o(.text.HAL_PWREx_DisableUCPDDeadBattery))
  [Called By]

  - >> HAL_MspInit

  HAL_RCCEx_PeriphCLKConfig (Thumb, 1114 bytes, Stack size 32 bytes, stm32g4xx_hal_rcc_ex.o(.text.HAL_RCCEx_PeriphCLKConfig))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_RCCEx_PeriphCLKConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_ADC_MspInit

  HAL_RCC_ClockConfig (Thumb, 806 bytes, Stack size 32 bytes, stm32g4xx_hal_rcc.o(.text.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 112
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ NVIC_EncodePriority
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  - >> RCC_GetSysClockFreqFromPLLSource
  - >> HAL_InitTick
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetSysClockFreq (Thumb, 252 bytes, Stack size 24 bytes, stm32g4xx_hal_rcc.o(.text.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCC_ClockConfig

  HAL_RCC_OscConfig (Thumb, 1974 bytes, Stack size 48 bytes, stm32g4xx_hal_rcc.o(.text.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 128
  - Call Chain = HAL_RCC_OscConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ NVIC_EncodePriority
  [Calls]
  - >> HAL_InitTick
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_SYSTICK_Config (Thumb, 16 bytes, Stack size 16 bytes, stm32g4xx_hal_cortex.o(.text.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_SYSTICK_Config ⇒ SysTick_Config ⇒ __NVIC_SetPriority
  [Calls]
  - >> SysTick_Config
  [Called By]
  - >> HAL_InitTick

  HAL_TIMEx_ConfigBreakDeadTime (Thumb, 304 bytes, Stack size 16 bytes, stm32g4xx_hal_tim_ex.o(.text.HAL_TIMEx_ConfigBreakDeadTime))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_TIMEx_ConfigBreakDeadTime
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIMEx_MasterConfigSynchronization (Thumb, 318 bytes, Stack size 20 bytes, stm32g4xx_hal_tim_ex.o(.text.HAL_TIMEx_MasterConfigSynchronization))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_TIMEx_MasterConfigSynchronization
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIMEx_OCN_Start (Thumb, 382 bytes, Stack size 48 bytes, stm32g4xx_hal_tim_ex.o(.text.HAL_TIMEx_OCN_Start))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_TIMEx_OCN_Start ⇒ TIM_CCxNChannelCmd
  [Calls]
  - >> TIM_CCxNChannelCmd
  [Called By]
  - >> DC_Init

  HAL_TIM_Base_Init (Thumb, 168 bytes, Stack size 16 bytes, stm32g4xx_hal_tim.o(.text.HAL_TIM_Base_Init))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_TIM_Base_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> HAL_TIM_Base_MspInit
  - >> TIM_Base_SetConfig
  [Called By]
  - >> MX_TIM17_Init

  HAL_TIM_Base_MspInit (Thumb, 58 bytes, Stack size 8 bytes, tim.o(.text.HAL_TIM_Base_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_TIM_Base_MspInit
  [Called By]
  - >> HAL_TIM_Base_Init

  HAL_TIM_MspPostInit (Thumb, 102 bytes, Stack size 40 bytes, tim.o(.text.HAL_TIM_MspPostInit))
  [Stack]

  - Max Depth = 84
  - Call Chain = HAL_TIM_MspPostInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIM_OC_ConfigChannel (Thumb, 196 bytes, Stack size 32 bytes, stm32g4xx_hal_tim.o(.text.HAL_TIM_OC_ConfigChannel))
  [Stack]

  - Max Depth = 52
  - Call Chain = HAL_TIM_OC_ConfigChannel ⇒ TIM_OC2_SetConfig
  [Calls]
  - >> TIM_OC2_SetConfig
  - >> TIM_OC6_SetConfig
  - >> TIM_OC5_SetConfig
  - >> TIM_OC4_SetConfig
  - >> TIM_OC3_SetConfig
  - >> TIM_OC1_SetConfig
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIM_OC_Init (Thumb, 168 bytes, Stack size 16 bytes, stm32g4xx_hal_tim.o(.text.HAL_TIM_OC_Init))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_TIM_OC_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> HAL_TIM_OC_MspInit
  - >> TIM_Base_SetConfig
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIM_OC_MspInit (Thumb, 58 bytes, Stack size 8 bytes, tim.o(.text.HAL_TIM_OC_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_TIM_OC_MspInit
  [Called By]
  - >> HAL_TIM_OC_Init

  HAL_TIM_OC_Start (Thumb, 606 bytes, Stack size 72 bytes, stm32g4xx_hal_tim.o(.text.HAL_TIM_OC_Start))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_TIM_OC_Start ⇒ TIM_CCxChannelCmd
  [Calls]
  - >> TIM_CCxChannelCmd
  [Called By]
  - >> DC_Init

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32g4xx_it.o(.text.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  MX_ADC1_Init (Thumb, 190 bytes, Stack size 64 bytes, adc.o(.text.MX_ADC1_Init))
  [Stack]

  - Max Depth = 348 + Unknown Stack Size
  - Call Chain = MX_ADC1_Init ⇒ HAL_ADC_ConfigChannel ⇒ LL_ADC_SetOffset
  [Calls]
  - >> HAL_ADC_ConfigChannel
  - >> HAL_ADCEx_MultiModeConfigChannel
  - >> HAL_ADC_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MX_GPIO_Init (Thumb, 186 bytes, Stack size 56 bytes, gpio.o(.text.MX_GPIO_Init))
  [Stack]

  - Max Depth = 100
  - Call Chain = MX_GPIO_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> main

  MX_TIM17_Init (Thumb, 60 bytes, Stack size 16 bytes, tim.o(.text.MX_TIM17_Init))
  [Stack]

  - Max Depth = 44
  - Call Chain = MX_TIM17_Init ⇒ HAL_TIM_Base_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> HAL_TIM_Base_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MX_TIM1_Init (Thumb, 246 bytes, Stack size 112 bytes, tim.o(.text.MX_TIM1_Init))
  [Stack]

  - Max Depth = 196 + Unknown Stack Size
  - Call Chain = MX_TIM1_Init ⇒ HAL_TIM_MspPostInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_TIM_MspPostInit
  - >> HAL_TIMEx_ConfigBreakDeadTime
  - >> HAL_TIM_OC_ConfigChannel
  - >> HAL_TIMEx_MasterConfigSynchronization
  - >> HAL_TIM_OC_Init
  - >> Error_Handler
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32g4xx_it.o(.text.MemManage_Handler))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  NMI_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32g4xx_it.o(.text.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32g4xx_it.o(.text.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32g4xx_it.o(.text.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  SysTick_Handler (Thumb, 8 bytes, Stack size 8 bytes, stm32g4xx_it.o(.text.SysTick_Handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = SysTick_Handler
  [Calls]
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32g431xx.o(RESET)

  SystemClock_Config (Thumb, 114 bytes, Stack size 88 bytes, main.o(.text.SystemClock_Config))
  [Stack]

  - Max Depth = 216 + Unknown Stack Size
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_OscConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ NVIC_EncodePriority
  [Calls]
  - >> HAL_RCC_ClockConfig
  - >> Error_Handler
  - >> HAL_RCC_OscConfig
  - >> HAL_PWREx_ControlVoltageScaling
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  SystemInit (Thumb, 18 bytes, Stack size 0 bytes, system_stm32g4xx.o(.text.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(.text)

  TIM_Base_SetConfig (Thumb, 406 bytes, Stack size 12 bytes, stm32g4xx_hal_tim.o(.text.TIM_Base_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_Base_SetConfig
  [Called By]
  - >> HAL_TIM_Base_Init
  - >> HAL_TIM_OC_Init

  TIM_CCxChannelCmd (Thumb, 54 bytes, Stack size 16 bytes, stm32g4xx_hal_tim.o(.text.TIM_CCxChannelCmd))
  [Stack]

  - Max Depth = 16
  - Call Chain = TIM_CCxChannelCmd
  [Called By]
  - >> HAL_TIM_OC_Start

  TIM_OC2_SetConfig (Thumb, 368 bytes, Stack size 20 bytes, stm32g4xx_hal_tim.o(.text.TIM_OC2_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_OC2_SetConfig
  [Called By]
  - >> HAL_TIM_OC_ConfigChannel

  UKSI_Calc_Init (Thumb, 176 bytes, Stack size 24 bytes, uksi_calc_res.o(.text.UKSI_Calc_Init))
  [Stack]

  - Max Depth = 92
  - Call Chain = UKSI_Calc_Init ⇒ HAL_ADC_Start ⇒ ADC_Enable ⇒ LL_ADC_GetCommonPathInternalCh
  [Calls]
  - >> HAL_ADCEx_Calibration_Start
  - >> HAL_ADC_Start
  - >> foster_set_mse
  - >> foster_init
  - >> ADC_ConfigFilter
  - >> ADC_ConfigCoef
  [Called By]
  - >> UKSI_Init

  UKSI_Calc_Isolation (Thumb, 236 bytes, Stack size 40 bytes, uksi_calc_res.o(.text.UKSI_Calc_Isolation))
  [Stack]

  - Max Depth = 80
  - Call Chain = UKSI_Calc_Isolation ⇒ foster_check
  [Calls]
  - >> foster_is_ready
  - >> foster_add_sample
  - >> ADC_Calc
  - >> foster_check
  [Called By]
  - >> UKSI_while

  UKSI_Init (Thumb, 48 bytes, Stack size 8 bytes, uksi_main.o(.text.UKSI_Init))
  [Stack]

  - Max Depth = 128
  - Call Chain = UKSI_Init ⇒ DC_Init ⇒ HAL_TIM_OC_Start ⇒ TIM_CCxChannelCmd
  [Calls]
  - >> UKSI_Calc_Init
  - >> DC_Init
  [Called By]
  - >> main

  UKSI_prewhile (Thumb, 2 bytes, Stack size 0 bytes, uksi_main.o(.text.UKSI_prewhile))
  [Called By]

  - >> main

  UKSI_while (Thumb, 332 bytes, Stack size 16 bytes, uksi_main.o(.text.UKSI_while))
  [Stack]

  - Max Depth = 96
  - Call Chain = UKSI_while ⇒ UKSI_Calc_Isolation ⇒ foster_check
  [Calls]
  - >> foster_check
  - >> UKSI_Calc_Isolation
  - >> DC_Enable
  [Called By]
  - >> main

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32g4xx_it.o(.text.UsageFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32g431xx.o(RESET)

  foster_add_sample (Thumb, 114 bytes, Stack size 8 bytes, foster_student.o(.text.foster_add_sample))
  [Stack]

  - Max Depth = 8
  - Call Chain = foster_add_sample
  [Called By]
  - >> UKSI_Calc_Isolation

  foster_check (Thumb, 374 bytes, Stack size 40 bytes, foster_student.o(.text.foster_check))
  [Stack]

  - Max Depth = 40
  - Call Chain = foster_check
  [Called By]
  - >> UKSI_while
  - >> UKSI_Calc_Isolation

  foster_init (Thumb, 90 bytes, Stack size 12 bytes, foster_student.o(.text.foster_init))
  [Stack]

  - Max Depth = 12
  - Call Chain = foster_init
  [Called By]
  - >> UKSI_Calc_Init

  foster_is_ready (Thumb, 40 bytes, Stack size 8 bytes, foster_student.o(.text.foster_is_ready))
  [Stack]

  - Max Depth = 8
  - Call Chain = foster_is_ready
  [Called By]
  - >> UKSI_Calc_Isolation

  foster_set_mse (Thumb, 44 bytes, Stack size 8 bytes, foster_student.o(.text.foster_set_mse))
  [Stack]

  - Max Depth = 8
  - Call Chain = foster_set_mse
  [Called By]
  - >> UKSI_Calc_Init

  main (Thumb, 48 bytes, Stack size 16 bytes, main.o(.text.main))
  [Stack]

  - Max Depth = 364 + Unknown Stack Size
  - Call Chain = main ⇒ MX_ADC1_Init ⇒ HAL_ADC_ConfigChannel ⇒ LL_ADC_SetOffset
  [Calls]
  - >> UKSI_while
  - >> UKSI_prewhile
  - >> UKSI_Init
  - >> MX_TIM1_Init
  - >> MX_TIM17_Init
  - >> MX_ADC1_Init
  - >> MX_GPIO_Init
  - >> SystemClock_Config
  - >> HAL_Init
  [Called By]
  - >> __rt_entry_main

  _fp_init (Thumb, 26 bytes, Stack size 0 bytes, fpinit.o(x$fpl$fpinit))
  [Called By]

  - >> __rt_lib_init_fp_1

  __fplib_config_fpu_vfp (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  __fplib_config_pureend_doubles (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  ### Local Symbols

  LL_ADC_IsDeepPowerDownEnabled (Thumb, 16 bytes, Stack size 4 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_IsDeepPowerDownEnabled))
  [Stack]

  - Max Depth = 4
  - Call Chain = LL_ADC_IsDeepPowerDownEnabled
  [Called By]
  - >> HAL_ADC_Init

  LL_ADC_DisableDeepPowerDown (Thumb, 24 bytes, Stack size 4 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_DisableDeepPowerDown))
  [Stack]

  - Max Depth = 4
  - Call Chain = LL_ADC_DisableDeepPowerDown
  [Called By]
  - >> HAL_ADC_Init

  LL_ADC_IsInternalRegulatorEnabled (Thumb, 16 bytes, Stack size 4 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_IsInternalRegulatorEnabled))
  [Stack]

  - Max Depth = 4
  - Call Chain = LL_ADC_IsInternalRegulatorEnabled
  [Called By]
  - >> HAL_ADC_Init

  LL_ADC_EnableInternalRegulator (Thumb, 30 bytes, Stack size 4 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_EnableInternalRegulator))
  [Stack]

  - Max Depth = 4
  - Call Chain = LL_ADC_EnableInternalRegulator
  [Called By]
  - >> HAL_ADC_Init

  LL_ADC_REG_IsConversionOngoing (Thumb, 16 bytes, Stack size 4 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_REG_IsConversionOngoing))
  [Stack]

  - Max Depth = 4
  - Call Chain = LL_ADC_REG_IsConversionOngoing
  [Called By]
  - >> HAL_ADC_Start
  - >> HAL_ADC_ConfigChannel
  - >> HAL_ADC_Init

  LL_ADC_IsEnabled (Thumb, 16 bytes, Stack size 4 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_IsEnabled))
  [Stack]

  - Max Depth = 4
  - Call Chain = LL_ADC_IsEnabled
  [Called By]
  - >> ADC_Enable
  - >> ADC_Disable
  - >> HAL_ADC_ConfigChannel
  - >> HAL_ADC_Init

  LL_ADC_SetCommonClock (Thumb, 26 bytes, Stack size 8 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_SetCommonClock))
  [Stack]

  - Max Depth = 8
  - Call Chain = LL_ADC_SetCommonClock
  [Called By]
  - >> HAL_ADC_Init

  LL_ADC_INJ_IsConversionOngoing (Thumb, 16 bytes, Stack size 4 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_INJ_IsConversionOngoing))
  [Stack]

  - Max Depth = 4
  - Call Chain = LL_ADC_INJ_IsConversionOngoing
  [Called By]
  - >> HAL_ADC_ConfigChannel
  - >> HAL_ADC_Init

  LL_ADC_IsDisableOngoing (Thumb, 16 bytes, Stack size 4 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_IsDisableOngoing))
  [Stack]

  - Max Depth = 4
  - Call Chain = LL_ADC_IsDisableOngoing
  [Called By]
  - >> ADC_Disable

  LL_ADC_Disable (Thumb, 28 bytes, Stack size 4 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_Disable))
  [Stack]

  - Max Depth = 4
  - Call Chain = LL_ADC_Disable
  [Called By]
  - >> ADC_Disable

  LL_ADC_GetMultimode (Thumb, 16 bytes, Stack size 4 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_GetMultimode))
  [Stack]

  - Max Depth = 4
  - Call Chain = LL_ADC_GetMultimode
  [Called By]
  - >> HAL_ADC_Start

  LL_ADC_REG_StartConversion (Thumb, 28 bytes, Stack size 4 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_REG_StartConversion))
  [Stack]

  - Max Depth = 4
  - Call Chain = LL_ADC_REG_StartConversion
  [Called By]
  - >> HAL_ADC_Start

  LL_ADC_Enable (Thumb, 28 bytes, Stack size 4 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_Enable))
  [Stack]

  - Max Depth = 4
  - Call Chain = LL_ADC_Enable
  [Called By]
  - >> ADC_Enable

  LL_ADC_GetCommonPathInternalCh (Thumb, 16 bytes, Stack size 4 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_GetCommonPathInternalCh))
  [Stack]

  - Max Depth = 4
  - Call Chain = LL_ADC_GetCommonPathInternalCh
  [Called By]
  - >> ADC_Enable
  - >> HAL_ADC_ConfigChannel

  LL_ADC_REG_SetSequencerRanks (Thumb, 58 bytes, Stack size 16 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_REG_SetSequencerRanks))
  [Stack]

  - Max Depth = 16
  - Call Chain = LL_ADC_REG_SetSequencerRanks
  [Called By]
  - >> HAL_ADC_ConfigChannel

  LL_ADC_SetChannelSamplingTime (Thumb, 54 bytes, Stack size 16 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_SetChannelSamplingTime))
  [Stack]

  - Max Depth = 16
  - Call Chain = LL_ADC_SetChannelSamplingTime
  [Called By]
  - >> HAL_ADC_ConfigChannel

  LL_ADC_SetSamplingTimeCommonConfig (Thumb, 26 bytes, Stack size 8 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_SetSamplingTimeCommonConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = LL_ADC_SetSamplingTimeCommonConfig
  [Called By]
  - >> HAL_ADC_ConfigChannel

  LL_ADC_SetOffset (Thumb, 60 bytes, Stack size 20 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_SetOffset))
  [Stack]

  - Max Depth = 20
  - Call Chain = LL_ADC_SetOffset
  [Called By]
  - >> HAL_ADC_ConfigChannel

  LL_ADC_SetOffsetSign (Thumb, 40 bytes, Stack size 16 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_SetOffsetSign))
  [Stack]

  - Max Depth = 16
  - Call Chain = LL_ADC_SetOffsetSign
  [Called By]
  - >> HAL_ADC_ConfigChannel

  LL_ADC_SetOffsetSaturation (Thumb, 40 bytes, Stack size 16 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_SetOffsetSaturation))
  [Stack]

  - Max Depth = 16
  - Call Chain = LL_ADC_SetOffsetSaturation
  [Called By]
  - >> HAL_ADC_ConfigChannel

  LL_ADC_GetOffsetChannel (Thumb, 30 bytes, Stack size 12 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_GetOffsetChannel))
  [Stack]

  - Max Depth = 12
  - Call Chain = LL_ADC_GetOffsetChannel
  [Called By]
  - >> HAL_ADC_ConfigChannel

  LL_ADC_SetOffsetState (Thumb, 40 bytes, Stack size 16 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_SetOffsetState))
  [Stack]

  - Max Depth = 16
  - Call Chain = LL_ADC_SetOffsetState
  [Called By]
  - >> HAL_ADC_ConfigChannel

  LL_ADC_SetChannelSingleDiff (Thumb, 52 bytes, Stack size 12 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_SetChannelSingleDiff))
  [Stack]

  - Max Depth = 12
  - Call Chain = LL_ADC_SetChannelSingleDiff
  [Called By]
  - >> HAL_ADC_ConfigChannel

  LL_ADC_SetCommonPathInternalCh (Thumb, 26 bytes, Stack size 8 bytes, stm32g4xx_hal_adc.o(.text.LL_ADC_SetCommonPathInternalCh))
  [Stack]

  - Max Depth = 8
  - Call Chain = LL_ADC_SetCommonPathInternalCh
  [Called By]
  - >> HAL_ADC_ConfigChannel

  LL_ADC_StartCalibration (Thumb, 40 bytes, Stack size 8 bytes, stm32g4xx_hal_adc_ex.o(.text.LL_ADC_StartCalibration))
  [Stack]

  - Max Depth = 8
  - Call Chain = LL_ADC_StartCalibration
  [Called By]
  - >> HAL_ADCEx_Calibration_Start

  LL_ADC_IsCalibrationOnGoing (Thumb, 14 bytes, Stack size 4 bytes, stm32g4xx_hal_adc_ex.o(.text.LL_ADC_IsCalibrationOnGoing))
  [Stack]

  - Max Depth = 4
  - Call Chain = LL_ADC_IsCalibrationOnGoing
  [Called By]
  - >> HAL_ADCEx_Calibration_Start

  LL_ADC_REG_IsConversionOngoing (Thumb, 16 bytes, Stack size 4 bytes, stm32g4xx_hal_adc_ex.o(.text.LL_ADC_REG_IsConversionOngoing))
  [Stack]

  - Max Depth = 4
  - Call Chain = LL_ADC_REG_IsConversionOngoing
  [Called By]
  - >> HAL_ADCEx_MultiModeConfigChannel

  LL_ADC_IsEnabled (Thumb, 16 bytes, Stack size 4 bytes, stm32g4xx_hal_adc_ex.o(.text.LL_ADC_IsEnabled))
  [Stack]

  - Max Depth = 4
  - Call Chain = LL_ADC_IsEnabled
  [Called By]
  - >> HAL_ADCEx_MultiModeConfigChannel

  RCC_GetSysClockFreqFromPLLSource (Thumb, 156 bytes, Stack size 24 bytes, stm32g4xx_hal_rcc.o(.text.RCC_GetSysClockFreqFromPLLSource))
  [Stack]

  - Max Depth = 24
  - Call Chain = RCC_GetSysClockFreqFromPLLSource
  [Called By]
  - >> HAL_RCC_ClockConfig

  __NVIC_SetPriorityGrouping (Thumb, 60 bytes, Stack size 12 bytes, stm32g4xx_hal_cortex.o(.text.__NVIC_SetPriorityGrouping))
  [Stack]

  - Max Depth = 12
  - Call Chain = __NVIC_SetPriorityGrouping
  [Called By]
  - >> HAL_NVIC_SetPriorityGrouping

  __NVIC_GetPriorityGrouping (Thumb, 16 bytes, Stack size 0 bytes, stm32g4xx_hal_cortex.o(.text.__NVIC_GetPriorityGrouping))
  [Called By]

  - >> HAL_NVIC_SetPriority

  NVIC_EncodePriority (Thumb, 108 bytes, Stack size 32 bytes, stm32g4xx_hal_cortex.o(.text.NVIC_EncodePriority))
  [Stack]

  - Max Depth = 32
  - Call Chain = NVIC_EncodePriority
  [Called By]
  - >> HAL_NVIC_SetPriority

  __NVIC_SetPriority (Thumb, 66 bytes, Stack size 8 bytes, stm32g4xx_hal_cortex.o(.text.__NVIC_SetPriority))
  [Stack]

  - Max Depth = 8
  - Call Chain = __NVIC_SetPriority
  [Called By]
  - >> SysTick_Config
  - >> HAL_NVIC_SetPriority

  SysTick_Config (Thumb, 82 bytes, Stack size 16 bytes, stm32g4xx_hal_cortex.o(.text.SysTick_Config))
  [Stack]

  - Max Depth = 24
  - Call Chain = SysTick_Config ⇒ __NVIC_SetPriority
  [Calls]
  - >> __NVIC_SetPriority
  [Called By]
  - >> HAL_SYSTICK_Config

  TIM_OC1_SetConfig (Thumb, 340 bytes, Stack size 20 bytes, stm32g4xx_hal_tim.o(.text.TIM_OC1_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_OC1_SetConfig
  [Called By]
  - >> HAL_TIM_OC_ConfigChannel

  TIM_OC3_SetConfig (Thumb, 366 bytes, Stack size 20 bytes, stm32g4xx_hal_tim.o(.text.TIM_OC3_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_OC3_SetConfig
  [Called By]
  - >> HAL_TIM_OC_ConfigChannel

  TIM_OC4_SetConfig (Thumb, 368 bytes, Stack size 20 bytes, stm32g4xx_hal_tim.o(.text.TIM_OC4_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_OC4_SetConfig
  [Called By]
  - >> HAL_TIM_OC_ConfigChannel

  TIM_OC5_SetConfig (Thumb, 210 bytes, Stack size 20 bytes, stm32g4xx_hal_tim.o(.text.TIM_OC5_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_OC5_SetConfig
  [Called By]
  - >> HAL_TIM_OC_ConfigChannel

  TIM_OC6_SetConfig (Thumb, 212 bytes, Stack size 20 bytes, stm32g4xx_hal_tim.o(.text.TIM_OC6_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_OC6_SetConfig
  [Called By]
  - >> HAL_TIM_OC_ConfigChannel

  TIM_CCxNChannelCmd (Thumb, 54 bytes, Stack size 16 bytes, stm32g4xx_hal_tim_ex.o(.text.TIM_CCxNChannelCmd))
  [Stack]

  - Max Depth = 16
  - Call Chain = TIM_CCxNChannelCmd
  [Called By]
  - >> HAL_TIMEx_OCN_Start

  ### Undefined Global Symbols