; Code Composer Project File, Version 2.0 (do not modify or remove this line)

[Project Settings]
ProjectDir="D:\project2833\Balsam_165_2020_04_12\"
ProjectType=Executable
CPUFamily=TMS320C28XX
Tool="Compiler"
Tool="CustomBuilder"
Tool="DspBiosBuilder"
Tool="Linker"
Config="Debug"
Config="Release"

[Source Files]
Source="Libraries\rts2800_fpu32.lib"
Source="Source\External\v120\DSP2833x_common\source\DSP2833x_Adc.c"
Source="Source\External\v120\DSP2833x_common\source\DSP2833x_ADC_cal.asm"
Source="Source\External\v120\DSP2833x_common\source\DSP2833x_CpuTimers.c"
Source="Source\External\v120\DSP2833x_common\source\DSP2833x_PieCtrl.c"
Source="Source\External\v120\DSP2833x_common\source\DSP2833x_SWPrioritizedDefaultIsr.c"
Source="Source\External\v120\DSP2833x_common\source\DSP2833x_SWPrioritizedPieVect.c"
Source="Source\External\v120\DSP2833x_common\source\DSP2833x_SysCtrl.c"
Source="Source\External\v120\DSP2833x_common\source\DSP2833x_usDelay.asm"
Source="Source\External\v120\DSP2833x_common\source\DSP2833x_Xintf.c"
Source="Source\External\v120\DSP2833x_headers\source\DSP2833x_GlobalVariableDefs.c"
Source="Source\Internal\ADC.c"
Source="Source\Internal\bios.c"
Source="Source\Internal\cntrl_adr.c"
Source="Source\Internal\crc16.c"
Source="Source\Internal\DAC.c"
Source="Source\Internal\ecan.c"
Source="Source\Internal\filter_bat2.c"
Source="Source\Internal\kanal.c"
Source="Source\Internal\log_to_mem.c"
Source="Source\Internal\main.c"
Source="Source\Internal\measure.c"
Source="Source\Internal\message.c"
Source="Source\Internal\peripher.c"
Source="Source\Internal\pulto.c"
Source="Source\Internal\RS485.c"
Source="Source\Internal\spise2p.c"
Source="Source\Internal\tools.c"
Source="F28335.cmd"
Source="Source\External\v120\DSP2833x_headers\cmd\DSP2833x_Headers_nonBIOS.cmd"

["Debug" Settings]
FinalBuildCmd=$(Proj_dir)\bin\hex2000.exe $(Proj_dir)\bin\UKSSTMS320F28335.out -boot -sci8 -map  $(Proj_dir)\bin\UKSSTMS320F28335.map -o $(Proj_dir)\bin\UKSSTMS320F28335.hex -i
FinalBuildCmd=$(Proj_dir)\bin\hex2000.exe $(Proj_dir)\bin\UKSSTMS320F28335.out -boot -sci8 -map  $(Proj_dir)\bin\UKSSTMS320F28335.map -o $(Proj_dir)\bin\UKSSTMS320F28335.bin -b

["Compiler" Settings: "Debug"]
Options=-g -pdsw225 -o0 -fr"$(Proj_dir)\Debug" -fs"$(Proj_dir)\Asm" -i"$(Proj_dir)\Source\External\v120\DSP2833x_headers\include" -i"$(Proj_dir)\Source\Internal\Include" -i"$(Proj_dir)\Source\External\v120\DSP2833x_common\include" -d"_DEBUG" -d"LARGE_MODEL" -md -ml -v28 --float_support=fpu32

["Compiler" Settings: "Release"]
Options=-pdsw225 -o3 -fr"$(Proj_dir)\Release" -d"LARGE_MODEL" -ml -v28

["Linker" Settings: "Debug"]
Options=-c -e_c_int00 -m"$(Proj_dir)\UKSSTMS320F28335.map" -o"$(Proj_dir)\bin\UKSSTMS320F28335.out" -stack0x3f0 -w -x -l"rts2800_fpu32.lib"

["Linker" Settings: "Release"]
Options=-c -m"$(Proj_dir)\Release\UKSSTMS320F28335.map" -o"$(Proj_dir)\Release\UKSSTMS320F28335.out" -w -x

["F28335.cmd" Settings: "Debug"]
LinkOrder=1

["F28335.cmd" Settings: "Release"]
LinkOrder=1

["Source\External\v120\DSP2833x_headers\cmd\DSP2833x_Headers_nonBIOS.cmd" Settings: "Debug"]
LinkOrder=2

["Source\External\v120\DSP2833x_headers\cmd\DSP2833x_Headers_nonBIOS.cmd" Settings: "Release"]
LinkOrder=1

